E-KLOZION	TECHNICAL RIDER 2026
RIDER TECHNIQUE
E-Klozion
DJ set · FR / EN
Advance technique : contact@e-klozion.music
FR - Rider technique
1. Format et balance
· DJ set.
· Installation et vérification environ 15 minutes avant le set.
· Technicien son présent ou joignable pendant le passage.
2. Régie préférée
· 2 x Pioneer CDJ-2000NXS2 ou CDJ-3000, firmware à jour.
· 1 x Pioneer DJM-900NXS2 ou DJM-A9.
· Lecteurs reliés en réseau.
· 2 retours DJ de puissance adaptée, placés de part et d'autre de la cabine.
3. Alternatives
· CDJ-2000NXS, XDJ-1000MK2, DJM-900NXS et autres configurations professionnelles peuvent être étudiés avec validation écrite préalable.
4. Son et cabine
· Système de diffusion professionnel adapté à la jauge.
· Régie stable, plane, dégagée, protégée du public et suffisamment éclairée.
· Lecteurs, table, réseau et moniteurs installés, câblés et testés avant l'arrivée.
· Eau à proximité et ventilation raisonnable si la cabine est chaude ou fermée.
5. Advance et captation
· Envoyer la fiche de régie, les horaires d'arrivée et de passage, ainsi que toute modification de matériel avant la date.
· Toute captation audio ou vidéo professionnelle doit être signalée avant la date.


TECHNICAL RIDER
E-Klozion
DJ set · EN
Technical advance: contact@e-klozion.music
EN - Technical rider
1. Format and line check
· DJ set.
· Setup and line check approximately 15 minutes before the set.
· Sound technician present or reachable during the performance.
2. Preferred booth
· 2 x Pioneer CDJ-2000NXS2 or CDJ-3000 with current firmware.
· 1 x Pioneer DJM-900NXS2 or DJM-A9.
· Players connected through Pro DJ Link.
· 2 adequately powered DJ booth monitors, one on each side.
3. Alternatives
· CDJ-2000NXS, XDJ-1000MK2, DJM-900NXS and other professional configurations may be considered with prior written approval.
4. Sound and booth
· Professional PA system suitable for the venue capacity.
· Stable, level, clear booth protected from the audience and sufficiently lit.
· Players, mixer, network and monitors installed, wired and tested before arrival.
· Water nearby and reasonable ventilation in warm or enclosed booths.
5. Advance and recording
· Send the venue technical specification, arrival and set times, and any proposed equipment change before the event.
· Any professional audio or video recording must be disclosed before the event.
Contact
E-Klozion · contact@e-klozion.music
contact@e-klozion.music  /  




